 ***Worldwide. Performance. Excellence.***

**Race Tires America, Inc**

*1545 Washington Street*

*Indiana, PA 15701*

*Tel: 724-349-7210*

TO: Dominion Raceway Late Model Teams

SUBJECT: TIRE INFO – McCreary Speed

**TIRE SPECIFICATIONS**



**AIR PRESSURE/SIZES**

* Tires are measured at the factory at 25 psi. 10 psi difference from right sides to left sides will equate to approximately ¾ of an inch of roll out difference cold. Expect approximately ¼ to ½ inch more of rollout hot.
* Pressure builds should be approximately 6-10 psi in right sides and 4-6 psi in left sides in greater than 20 lap runs.
* Recommended minimum cold air pressure is 23-25 psi for right sides and 13-15 psi for left sides.

**SPRING RATE**



Spring Rate is defined as the amount of load (force) in pounds required to deflect a tire one (1) inch at a given pressure (psi).

**MOUNTING PROCEDURE RECOMMENDATION**

The McCreary Speed is marked with a direction arrow in order to minimize any issues with the tread splice in service. Tires should be mounted with arrow pointing toward the front of the car.

If you have any other questions please contact us at American Racer at 724-349-7210 and ask for Scott Junod or Levi Sikora.

Thank you for racing at Dominion Raceway.

American Racer